
State Machine - |DE2_Media_Computer|nios_system:NiosII|Char_LCD_16x2:the_Char_LCD_16x2|s_lcd_controller
Name s_lcd_controller.LCD_STATE_6_COMPLETE s_lcd_controller.LCD_STATE_5_TRANSFER s_lcd_controller.LCD_STATE_4_BEGIN_TRANSFER s_lcd_controller.LCD_STATE_3_CHECK_BUSY s_lcd_controller.LCD_STATE_2_START_CHECK_BUSY s_lcd_controller.LCD_STATE_1_INITIALIZE s_lcd_controller.LCD_STATE_0_IDLE 
s_lcd_controller.LCD_STATE_0_IDLE 0 0 0 0 0 0 0 
s_lcd_controller.LCD_STATE_1_INITIALIZE 0 0 0 0 0 1 1 
s_lcd_controller.LCD_STATE_2_START_CHECK_BUSY 0 0 0 0 1 0 1 
s_lcd_controller.LCD_STATE_3_CHECK_BUSY 0 0 0 1 0 0 1 
s_lcd_controller.LCD_STATE_4_BEGIN_TRANSFER 0 0 1 0 0 0 1 
s_lcd_controller.LCD_STATE_5_TRANSFER 0 1 0 0 0 0 1 
s_lcd_controller.LCD_STATE_6_COMPLETE 1 0 0 0 0 0 1 

State Machine - |DE2_Media_Computer|nios_system:NiosII|Char_LCD_16x2:the_Char_LCD_16x2|altera_up_character_lcd_initialization:Char_LCD_Init|s_lcd_initialize
Name s_lcd_initialize.LCD_INIT_STATE_3_DONE s_lcd_initialize.LCD_INIT_STATE_2_CHECK_DONE s_lcd_initialize.LCD_INIT_STATE_1_SEND_COMMAND s_lcd_initialize.LCD_INIT_STATE_0_WAIT_POWER_UP 
s_lcd_initialize.LCD_INIT_STATE_0_WAIT_POWER_UP 0 0 0 0 
s_lcd_initialize.LCD_INIT_STATE_1_SEND_COMMAND 0 0 1 1 
s_lcd_initialize.LCD_INIT_STATE_2_CHECK_DONE 0 1 0 1 
s_lcd_initialize.LCD_INIT_STATE_3_DONE 1 0 0 1 

State Machine - |DE2_Media_Computer|nios_system:NiosII|Char_LCD_16x2:the_Char_LCD_16x2|altera_up_character_lcd_communication:Char_LCD_Comm|s_lcd
Name s_lcd.LCD_STATE_0_OPERATION s_lcd.LCD_STATE_3_END s_lcd.LCD_STATE_2_HOLD s_lcd.LCD_STATE_1_ENABLE s_lcd.LCD_STATE_4_IDLE 
s_lcd.LCD_STATE_4_IDLE 0 0 0 0 0 
s_lcd.LCD_STATE_1_ENABLE 0 0 0 1 1 
s_lcd.LCD_STATE_2_HOLD 0 0 1 0 1 
s_lcd.LCD_STATE_3_END 0 1 0 0 1 
s_lcd.LCD_STATE_0_OPERATION 1 0 0 0 1 

State Machine - |DE2_Media_Computer|nios_system:NiosII|AV_Config:the_AV_Config|s_serial_transfer
Name s_serial_transfer.STATE_6_POST_READ s_serial_transfer.STATE_5_READ_TRANSFER s_serial_transfer.STATE_4_PRE_READ s_serial_transfer.STATE_3_POST_WRITE s_serial_transfer.STATE_2_WRITE_TRANSFER s_serial_transfer.STATE_1_PRE_WRITE s_serial_transfer.STATE_0_IDLE 
s_serial_transfer.STATE_0_IDLE 0 0 0 0 0 0 0 
s_serial_transfer.STATE_1_PRE_WRITE 0 0 0 0 0 1 1 
s_serial_transfer.STATE_2_WRITE_TRANSFER 0 0 0 0 1 0 1 
s_serial_transfer.STATE_3_POST_WRITE 0 0 0 1 0 0 1 
s_serial_transfer.STATE_4_PRE_READ 0 0 1 0 0 0 1 
s_serial_transfer.STATE_5_READ_TRANSFER 0 1 0 0 0 0 1 
s_serial_transfer.STATE_6_POST_READ 1 0 0 0 0 0 1 

State Machine - |DE2_Media_Computer|nios_system:NiosII|AV_Config:the_AV_Config|altera_up_av_config_serial_bus_controller:Serial_Bus_Controller|s_serial_protocol
Name s_serial_protocol.STATE_5_STOP_BIT s_serial_protocol.STATE_4_TRANSFER s_serial_protocol.STATE_3_START_BIT s_serial_protocol.STATE_2_RESTART_BIT s_serial_protocol.STATE_1_INITIALIZE s_serial_protocol.STATE_0_IDLE 
s_serial_protocol.STATE_0_IDLE 0 0 0 0 0 0 
s_serial_protocol.STATE_1_INITIALIZE 0 0 0 0 1 1 
s_serial_protocol.STATE_2_RESTART_BIT 0 0 0 1 0 1 
s_serial_protocol.STATE_3_START_BIT 0 0 1 0 0 1 
s_serial_protocol.STATE_4_TRANSFER 0 1 0 0 0 1 
s_serial_protocol.STATE_5_STOP_BIT 1 0 0 0 0 1 
